,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##
ZRNU073L1GA,270/230/200,-,L1,32,7500,2.20,27-9/16 x 7-1/2 x 27-9/16,700 x 190 x 700,-,BLDC,Sirocco,2500,2.50,0.5,15,ZRNU073L1GA,16.3,35.9,1-1/4,32,3/8,9.52,1/4,6.35,31/28/24,-,"1, 208-230, 60",9.52,6.35,R32,0.4,27/26/23,Low Static Duct
ZRNU093L1GA,320/250/200,-,L1,32,9600,2.80,30-1/2 x 7-1/2 x 27-9/16,700 x 190 x 700,-,BLDC,Sirocco,3200,3.20,0.5,15,ZRNU093L1GA,16.3,35.9,1-1/4,32,3/8,9.52,1/4,6.35,31/28/24,-,"1, 208-230, 60",9.52,6.35,R32,0.4,30/26/23,Low Static Duct
