,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Indoor Unit Total Capacity##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_High Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_High Gas Side (Heat Recovery)(mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZRUN024GSS0,U36A,2 x 18,Hermetically Sealed Scroll,24000,-,37-13/32 x 32-27/32 x 13,950 x 834 x 330,2119,-,0.124 x 1,Propeller,27000,-,-,26.4,ZRUN024GSS0,-,148,5/8,15.88,-,-,3/8,9.52,-,-,1.62,1.98,"1, 208-230,60",-,3.3,15.88,9.52,R32,50,52,-,23~122 (DB),-,-13~61 (WB),Multi V S R32
