,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Charge (oz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Type##other##,Continuous Operation Range (Cooling)(C)##other##,Continuous Operation Range (Cooling)(F)##other##,Continuous Operation Range (Heating)(C)##other##,Continuous Operation Range (Heating)(F)##other##
LMU483HV,LMU483HV,U60A,-,Scroll,10800~48000~58000,3.17~14.07~17,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",Electronic Expansion Valve,"1,942 x 2",55 x 2,124.2 x 2,BLDC,Propeller x 2,3.64~15.83~17.29,12420~54000~59000,A8UW48GFA3,88,194,3/4 ,19.05 ,3/8 ,9.52 ,0.664~3.75~5.201,0.747~4.522~5.277,"1, 208-230 , 60",3 x 8 (4.0),4200,148.2,19.05,9.52,R410A,3~17~23.6,3.4~20.5~23.9,-,-,53,55,Multi F MAX,-10~48,14.0~118,-20~18,-4.0~64
LMU543HV,LMU543HV,U60A,-,Scroll,10800~50500~63200,3.17~14.8~18.52,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",Electronic Expansion Valve,"1,942 x 2",55 x 2,124.2 x 2,BLDC,Propeller x 2,3.64~17~18.76,12420~58000~64000,A8UW54GFA3,88,194,3/4 ,19.05 ,3/8 ,9.52 ,0.664~4.008~5.709,0.747~5.074~5.825,"1, 208-230 , 60",3 x 8 (4.0),4200,148.2,19.05,9.52,R410A,3~18.2~25.9,3.4~23~26.4,-,-,53,55,Multi F MAX,-10~48,14.0~118,-20~18,-4.0~64
