,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x H x D) (mm)##other##,Dimensions (W x H x D) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"LSN303HLV3",Wall Mounted,LSN303HLV3,S4NW30R43FA,SR,1200 x 360 x 265,47-1/4 x 14-3/16 x 10-7/16,15.0,19/32,20.0,25/32,15.88,5/8,9.52,3/8,1_208/230_60,4 x 1.0,4 x 16,12,13,31 / 25 / 21 / 17,1095 / 883 / 742 / 601,33 / 27 / 23 / 19,1166 / 954 / 813 / 671,8.79,30000,9.53,32500,2655,2754,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,110,18.5,40.8,R410A,- / 51 / 47 / 43 / 33,- / 51 / 47 / 43
"LSN363HLV3",Wall Mounted,LSN363HLV3,S4NW36R43FA,SR,1200 x 360 x 265,47-1/4 x 14-3/16 x 10-7/16,15.0,19/32,20.0,25/32,15.88,5/8,9.52,3/8,1_208/230_60,4 x 1.0,4 x 16,15,14,31 / 25 / 21 / 17,1095 / 883 / 742 / 601,33 / 27 / 23 / 19,1166 / 954 / 813 / 671,9.67,33000,10.32,35200,3300,3115,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,110,18.5,40.8,R410A,- / 51 / 47 / 43 / 33,- / 51 / 47 / 43
