,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"LSN181HSV5",Wall Mounted,LSN181HSV5,S4NW18K41DA,SK,998 x 345 x 210,39-9/32 x 13-19/32 x 8-9/32,16.0,5/8,21.5,27/32,15.88,5/8,9.52,3/8,1_208/230_60,4 x 1.0,4 x 18,6.3,8.2,20.0 / 15.0 / 13.5 / 10.5,706 / 530 / 477 / 371,20.0 / 15.5 / 14.0 / 10.5,706 / 547 / 494 / 371,5.28,"18,000",6.33,"21,600","1,431","1,730",Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,70,11.6,25.6,R410A,- / 47 / 42 / 37 / 31,- / 47 / 42 / 37