,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
KUSXB361A,KUSXB361A,U60A,BLDC,R1 Scroll,33000,9.7,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,40000,11.7,ZUUR36GA0,86.3,190.2,5/8,15.88,3/8 ,9.52 ,2.8,3.3,"1,208-230,60",3 x 10,15.88,9.52 ,R32,12.3,14.5,65,-,52,54,-15~48,5~118,-20~18,-4~64,Single_R32_ODU
KUSXB421A,KUSXB421A,U60A,BLDC,R1 Scroll,42000,12.3,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,46000,13.5,ZUUR42GA0,86.3,190.2,5/8,15.88,3/8 ,9.52 ,3.59,4.01,"1,208-230,60",3 x 10,15.88,9.52 ,R32,15.8,17.6,71,-,54,56,-15~48,5~118,-20~18,-4~64,Single_R32_ODU
KUSXB481A,KUSXB481A,U60A,BLDC,R1 Scroll,45500,13.3,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,50000,14.7,ZUUR48GA0,86.3,190.2,5/8,15.88,3/8 ,9.52 ,3.89,4,"1,208-230,60",3 x 10,15.88,9.52 ,R32,17.1,17.6,71,-,54,56,-15~48,5~118,-20~18,-4~64,Single_R32_ODU
KUSXB601A,KUSXB601A,U60A,BLDC,R1 Scroll,52500,15.4,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,56500,16.6,ZUUR60GA0,86.3,190.2,3/4,19.05,3/8 ,9.52 ,4.38,4.38,"1,208-230,60",3 x 10,19.05,9.52 ,R32,19.2,19.2,71,-,54,56,-15~48,5~118,-20~18,-4~64,Single_R32_ODU
