,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Charge (oz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
KUSXA121A,KUSXA121A,U36A,BLDC,R1 Scroll,12500,3.7,37-13/32 x 32-27/32 x 13,950 x 834 x 330,EEV,2048,58,124 x 1,BLDC,Axial x 1,15000,4.4,ZUUR12GH0,64.3,141.1,3/8,9.52,1/4,6.35,0.94,1.11,"1,208-230,60",3 x 12,9.52,6.35,R32,4.1,4.9,67,-,51,52,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
KUSXA181A,KUSXA181A,U36A,BLDC,R1 Scroll,18000,5.3,37-13/32 x 32-27/32 x 13,950 x 834 x 330,EEV,2048,58,124 x 1,BLDC,Axial x 1,20000,5.9,ZUUR18GH0,64.3,141.1,5/8,15.88,3/8,9.52,1.33,1.54,"1,208-230,60",3 x 12,15.88,9.52,R32,5.9,6.8,67,-,51,52,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
KUSXA241A,KUSXA241A,U36A,BLDC,R1 Scroll,24000,7,37-13/32 x 32-27/32 x 13,950 x 834 x 330,EEV,2048,58,124 x 1,BLDC,Axial x 1,27000,7.9,ZUUR24GH0,64.3,141.1,5/8,15.88,3/8,9.52,1.92,2.08,"1,208-230,60",3 x 12,15.88,9.52,R32,8.4,9.1,67,-,51,52,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
