,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Refrigerant Charge (oz)##other##
LMU183HV,LMU183HV,U24A,-,Twin Rotary,18000,5.27,34-1/4 x 25-19/32 x 13,870 x 650 x 330,Electronic Expansion Valve,1766,50,85.4 x 1,BLDC,Axial,22000,6.44,LMU183HV,45.8,101,3/8 x 2,9.52 x 2,1/4 x 2,6.35 x 2,1.3,1.7,"1, 208-230 , 60",3 x 12 (3.3),1800,9.52,6.35,R410A,6.03,8.11,63,65,48,53,-10~48,14~118,-20~18,-4~64,MULTI F,63.5

