,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##
ZRNU483M3AA,"1,413/1,201/989",-,M3,32,"48,100",14.10,49-7/32 x 14-3/16 x 27-9/16,1250 x 360 x 700,500,BLDC,Sirocco Fan,15900,15.9,3.2,15,ZRNU483M3AA,42.5,93.7,1-1/4,32,5/8,15.88,3/8,9.52,172 / 102 / 75,-,"1, 208-230, 60",15.88,9.52,R32,2.5,42/39/37,Middle Static Duct
ZRNU543M3AA,"1,766/1,589/1,413",-,M3,32,"54,000",15.80,49-7/32 x 14-3/16 x 27-9/16,1250 x 360 x 700,500,BLDC,Sirocco Fan,18000,18.0,3.2,15,ZRNU543M3AA,42.5,93.7,1-1/4,32,5/8,15.88,3/8,9.52,260 / 215 / 172,-,"1, 208-230, 60",15.88,9.52,R32,2.5,44/43/42,Middle Static Duct
