,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"LSN180HEV2",Wall Mounted,LSN180HEV2,S4NW18K23AB,SK,998 x 345 x 210,39-9/32 x 13-19/32 x 8-9/32,16.0,5/8,21.5,27/32,12.7,1/2,6.35,1/4,1_208/230_60,4 x 1.0,4 x 18,6.90,7.60,19.5 / 14.5 / 13.0 / 10.5,689 / 512 / 459 / 371,18.5 / 16.0 / 13.5 / 11.0,653 / 565 / 477 / 388,5.28,"18,000",5.57,"19,000","1,500","1,583",Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,58,11.8,26,R410A,- / 48 / 43 / 38 / 32,- / 48 / 43 / 38
"LSN240HEV2",Wall Mounted,LSN240HEV2,S4NW24K23AC,SK,998 x 345 x 210,39-9/32 x 13-19/32 x 8-9/32,16.0,5/8,21.5,27/32,12.7,1/2,6.35,1/4,1_208/230_60,4 x 1.0,4 x 18,9.00,9.00,19.5 / 14.5 / 13.0 / 10.5,689 / 512 / 459 / 371,18.5 / 16.0 / 13.5 / 11.0,653 / 565 / 477 / 388,6.45,"22,000",6.45,"22,000","2,000","1,930",Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,58,11.8,26,R410A,- / 48 / 43 / 38 / 32,- / 48 / 43 / 38

