,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
KUSXA301A,KUSXA301A,U60A,BLDC,R1 Scroll,30000,8.8,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,34000,10,ZUUR30GH0,86.3,190.2,5/8,15.88,3/8 ,9.52 ,2.22,2.49,"1,208-230,60",3 x 10,15.88,9.52 ,R32,9.8,10.9,69,-,52,54,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
KUSXA361A,KUSXA361A,U60A,BLDC,R1 Scroll,33000,9.7,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,40000,11.7,ZUUR36GH0,86.3,190.2,5/8,15.88,3/8 ,9.52 ,2.54,3.09,"1,208-230,60",3 x 10,15.88,9.52 ,R32,11.1,13.5,69,-,52,54,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
KUSXA422A,KUSXA422A,U60A,BLDC,R1 Scroll,42000,12.3,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,46000,13.5,ZUUR42GH0,98.7,217.6,5/8,15.88,3/8 ,9.52 ,3.36,3.64,"1,208-230,60",3 x 10,15.88,9.52 ,R32,14.8,16,71,-,54,56,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
KUSXA482A,KUSXA482A,U60A,BLDC,R1 Scroll,46000,13.5,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,1942 x 2,55 x 2,124 x 2,BLDC,Axial x 2,50000,14.7,ZUUR48GH0,98.7,217.6,5/8,15.88,3/8 ,9.52 ,3.74,3.76,"1,208-230,60",3 x 10,15.88,9.52 ,R32,16.4,16.5,71,-,54,56,-15~48,5~118,-20~18,-4~64,Single R32 ODU(RED)
