,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
LUU180HV,LUU180HV,U36A,-,Twin Rotary,18000,-,37-13/32 x 32-27/32 x 12-31/32,950 x 834 x 330,EEV,2048,-,-,Brushless Digitally Controlled,Propeller,18500,-,LUU180HV,-,61.5,3/8,9.52,5/8,15.88,1.43,1.62,"1,208-230,60",4x14,15.88,9.52,R410A,-,-,-,-,48,52,-,5~118,-,-4~64,SingleZone
LUU240HV,LUU240HV,U36A,-,Twin Rotary,23000,-,37-13/32 x 32-27/32 x 12-31/32,950 x 834 x 330,EEV,2048,-,-,Brushless Digitally Controlled,Propeller,27000,-,LUU240HV,-,64.2,3/8,9.52,5/8,15.88,1.95,2.1,"1,208-230,60",4x14,15.88,9.52,R410A,-,-,-,-,48,52,-,5~118,-,-4~64,SingleZone
