,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x H x D) (mm)##other##,Dimensions (W x H x D) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"LAN090HYV3",Wall Mounted,LAN090HYV3,S4NW09K21FA,SK,998 x 345 x 210,39-9/32 x 13-19/32 x 8-9/32,15.0,19/32,20.0,25/32,9.52,3/8,6.35,1/4,1_208/230_60,4 x 1.0,4 x 16,3,4,15.0 / 12.0 / 10 / 5.2,530 / 424 / 353 / 184,15.0 / 12.0 / 10 / 5.2,530 / 424 / 353 / 184,2.64,9000,3.22,11000,570,710,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,58,11.4,25.1,R410A,- / 42 / 36 / 26 / 22,- / 42 / 36 / 26
"LAN120HYV3",Wall Mounted,LAN120HYV3,S4NW12K21FA,SK,998 x 345 x 210,39-9/32 x 13-19/32 x 8-9/32,15.0,19/32,20.0,25/32,9.52,3/8,6.35,1/4,1_208/230_60,4 x 1.0,4 x 16,4,4.5,15.0 / 12.0 / 10 / 5.2,530 / 424 / 353 / 184,15.0 / 12.0 / 10 / 5.2,530 / 424 / 353 / 184,3.52,12000,3.99,13600,870,970,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,58,11.4,25.1,R410A,- / 42 / 36 / 26 / 22,- / 42 / 36 / 26