,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Dehumidification Rate (pts./hr.)##other##,Factory Set (High) External Static Pressure (in.wg)##other##,Maximum External Static Pressure (in. wg)##other##,Type##other##
LHN248HV1,LHN248HV1,706/547/459,-,MA,32,24000,7.1,43-5/16 x 12-7/32 x 30-7/16,900x245x691 ,165,BLDC,Sirocco,27000,-,AMNW24GMAA0,29.1,64.2,"1-1/4(O.D.), 31/32(I.D.)","32(O.D.), 25(I.D.)",1/2,12.7,1/4,6.35 ,4 x 18 (No. x AWG)^2,-,-,"1, 208-230, 60",12.7,6.35 ,R410A,1.7,57,38/33/30,-,3.68,0.24,0.59,MSP Duct
LHN188HV1,LHN188HV1,635/530/424,-,MA,32,18000,5.6,43-5/16 x 12-7/32 x 30-7/16,900x245x691 ,165,BLDC,Sirocco,20000,-,AMNW18GMAA0,27.9,61.5,"1-1/4(O.D.), 31/32(I.D.)","32(O.D.), 25(I.D.)",1/2,12.7,1/4,6.35 ,4 x 18 (No. x AWG)^2,-,-,"1, 208-230, 60",12.7,6.35 ,R410A,1.7,54,36/32/29,-,3.68,0.24,0.59,MSP Duct
LHN128HV1,LHN128HV1,494/424/353,-,MA,32,12000,3.6,43-5/16 x 12-7/32 x 30-7/16,900x245x691 ,165,BLDC,Sirocco,15000,-,AMNW12GMAA0,27.9,61.5,"1-1/4(O.D.), 31/32(I.D.)","32(O.D.), 25(I.D.)",1/2,12.7,1/4,6.35 ,4 x 18 (No. x AWG)^2,-,,"1, 208-230, 60",12.7,6.35 ,R410A,1.7,47,31/29/28,-,3.68,0.24,0.59,MSP Duct
LHN098HV1,LHN098HV1,353/318/283,-,MA,32,9000,2.8,43-5/16 x 12-7/32 x 30-7/16,900x245x691 ,165,BLDC,Sirocco,12000,-,AMNW09GMAA0,27.9,61.5,"1-1/4(O.D.), 31/32(I.D.)","32(O.D.), 25(I.D.)",1/2,12.7,1/4,6.35 ,4 x 18 (No. x AWG)^2,-,,"1, 208-230, 60",12.7,6.35 ,R410A,1.7,44,28/27/26,-,3.68,0.24,0.59,MSP Duct
