,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Minimum Circuit Ampacity (MCA) (A)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"LSU180HEV2",Wall Mounted,LSU180HEV2,S4UW18K23AB,U24A,870 x 650 x 330,34-1/4 x 25-19/32 x 13,12.7,1/2,6.35,1/4,15,20,1_208/230_60,3 x 2.5,3 x 12,4 x 1.0,4 x 18,6.90,7.60,49,1730,5.28,"18,000",5.57,"19,000","1,500","1,583",Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,10,32.8,44.5,98.1,-10 ~ 48 (DB),14 ~ 118.4 (DB),-10 ~ 18.3 (WB),14 ~ 65 (WB),3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1350,47.6,24,0.26,55,55
"LSU240HEV2",Wall Mounted,LSU240HEV2,S4UW24K23AC,U24A,870 x 650 x 330,34-1/4 x 25-19/32 x 13,12.7,1/2,6.35,1/4,15,20,1_208/230_60,3 x 2.5,3 x 12,4 x 1.0,4 x 18,9.00,9.00,49,1730,6.45,"22,000",6.45,"22,000","2,000","1,930",Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,10,32.8,44.5,98.1,-10 ~ 48 (DB),14 ~ 118.4 (DB),-10 ~ 18.3 (WB),14 ~ 65 (WB),3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1350,47.6,24,0.26,55,55

