,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##
"ARNU183TTD4",470 / 427 / 385,13.31 / 12.09 / 10.9,TT,25.4,19100,5.6,46-1/2 x 17-3/4 x 6-7/8,-,-,-,Cross Flow,21500,6.3,0.38,-,ARNU183TTD4,19.05,42,1,25.4,1/2,12.7,1/4,6.35,70,70,"1,208/230,60",12.7,6.35,R410A,0.3,40 / 37 / 35  ,1Way CST
"ARNU243TTD4",515 / 470 / 406,14.58 / 13.31 / 11.5,TT,25.4,24200,7.09,46-1/2 x 17-3/4 x 6-7/8,-,-,-,Cross Flow,24200,7.9,0.38,-,ARNU243TTD4,19.05,42,1,25.4,5/8,15.88,3/8,9.52,70,70,"1,208/230,60",15.88,9.52,R410A,0.3,43 / 40 / 36  ,1Way CST

