,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##
"ARNU073TUD4",290 / 258 / 226,8.21 / 7.31 / 6.4,TU,25.4,7500,2.2,33-7/8 x 17-3/4 x 6-11/16,-,-,-,Cross Flow,8500,2.49,0.23,-,ARNU073TUD4,14.97,33,1,25.4,1/2,12.7,1/4,6.35,40,40,"1,208/230,60",12.7,6.35,R410A,0.18,32 / 29 / 25  ,1Way CST
"ARNU093TUD4",325 / 304 / 290,9.2 / 8.61 / 8.21,TU,25.4,9600,2.81,33-7/8 x 17-3/4 x 6-11/16,-,-,-,Cross Flow,10900,3.19,0.23,-,ARNU093TUD4,14.97,33,1,25.4,1/2,12.7,1/4,6.35,40,40,"1,208/230,60",12.7,6.35,R410A,0.18,35 / 34 / 32  ,1Way CST
"ARNU123TUD4",353 / 325 / 290,10 / 9.2 / 8.21,TU,25.4,12300,3.6,33-7/8 x 17-3/4 x 6-11/16,-,-,-,Cross Flow,13600,3.99,0.23,-,ARNU123TUD4,14.97,33,1,25.4,1/2,12.7,1/4,6.35,40,40,"1,208/230,60",12.7,6.35,R410A,0.18,38 / 35 / 32  ,1Way CST

