,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Dehumidification Rate (pts./hr.)##other##,Factory Set (High) External Static Pressure (in.wg)##other##,Maximum External Static Pressure (in. wg)##other##,Type##other##
KNUJB091A,KNUJB091A,353.1 / 317.8 / 282.5,10 / 9 / 8,MA,32,9000,2.6,35-7/16 x 9-21/32 x 27-9/16,900x245x700,165,-,Sirocco,13500,4.0,ZMNR09GMAA0,28,61.7,"1-1/4(O.D.), 1(I.D.)","32(O.D.), 25.4(I.D.)",3/8,9.52,1/4,6.35 ,-,-,-,"1, 208-230, 60",9.52,6.35 ,R32,3.2,65,47,51,-,-,-,Mid Static Ducted
KNUJB121A,KNUJB121A,494.4 / 423.8 / 353.1,14 / 12 / 10,MA,32,12000,3.5,35-7/16 x 9-21/32 x 27-9/16,900x245x700,165,-,Sirocco,15000,4.4,ZMNR12GMAA0,28,61.7,"1-1/4(O.D.), 1(I.D.)","32(O.D.), 25.4(I.D.)",3/8,9.52,1/4,6.35 ,-,-,-,"1, 208-230, 60",9.52,6.35 ,R32,4.4,65,49,52,-,-,-,Mid Static Ducted
KNUJB181A,KNUJB181A,635.7 / 529.7 / 423.8,-,MA,32,18000,5.3,35-7/16 x 9-21/32 x 27-9/16,900x245x700,165,-,Sirocco,20000,5.9,ZMNR18GMAA0,27.9,61.5,"1-1/4(O.D.), 1(I.D.)","32(O.D.), 25.4(I.D.)",5/8,15.88,3/8,9.52,-,-,-,"1, 208-230, 60",15.88,9.52,R32,6.4,65,48,52,-,-,-,Mid Static Ducted
KNUJB241A,KNUJB241A,706.3 / 547.4 / 459.1,-,MA,32,2300,6.7,35-7/16 x 9-21/32 x 27-9/16,900x245x700,165,-,Sirocco,27000,7.9,ZMNR24GMAA0,29.1,64.2,"1-1/4(O.D.), 1(I.D.)","32(O.D.), 25.4(I.D.)",5/8,15.88,3/8,9.52,-,-,-,"1, 208-230, 60",15.88,9.52,R32,8.6,65,48,52,-,-,-,Mid Static Ducted
