,Normal Capacity (CMH)##other##,Normal Capacity (CFM)##other##,Power Supply (Ph_V_Hz)##other##,ERV Mode Current (SH/H/L)(A)##other##,ERV Mode Power Input (SH/H/L)(W)##other##,ERV Mode Air Flow (SH/H/L)(CMH)##other##,ERV Mode Air Flow (SH/H/L)(CFM)##other##,ERV Mode External static pressure (SH/H/L)(Pa)##other##,ERV Mode Sound pressure level (SH/H/L)(dB(A))##other##,Bypass Mode Current (SH/H/L)(A)##other##,Bypass Mode Power Input (SH/H/L)(W)##other##,Bypass Mode Air Flow (SH/H/L)(CMH)##other##,Bypass Mode Air Flow (SH/H/L)(CFM)##other##,Bypass Mode External static pressure (SH/H/L)(Pa)##other##,Bypass Mode Sound pressure level (SH/H/L)(dB(A))##other##,Heat Exchanger type##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Dimensions (WxHxD)(mm)##other##,Dimensions (WxHxD)(inch)##other##,Duct work Qty(EA)##other##,Duct work Size(Ph)(mm)##other##,Duct work Size(Ph)(inch)##other##,Supply Air Fan Qty (EA)##other##,Supply Air Fan Type##other##,Exhaust Air Fan Qty (EA)##other##,Exhaust Air Fan Type##other##,Filters Qty (EA)##other##,Filters Type##other##,Filters Size (WxHxD)(mm)##other##,Filters Size (WxHxD)(inch)##other##,Operation Range (Outdoor Temperature)(C DB(F DB))##other##,Wiring Connections Power Supply Cable (No x mm2 (AWG))##other##,Temperature Exchange Efficiency (AHRI condition) Cooling (%)##other##,Temperature Exchange Efficiency (AHRI condition) Heating (%)##other##,Enthalpy Exchange Efficiency (AHRI condition) Cooling (%)##other##,Enthalpy Exchange Efficiency (AHRI condition) Heating (%)##other##,Type##other##,Chassis name##other##,Model name##other##,Model name(Factory)##other##
ARV00903RA6,150,90,"1, 208/230, 60",0.44 / 0.40 / 0.26,54.3 / 47.6 / 27.9,150 / 150 / 80,90 / 90 / 47,100 / 70 / 50,28 / 26 / 21,0.50 / 0.44 / 0.29,62.6 / 53.8 / 31.9,150 / 150 / 80,90 / 90 / 47,100 / 70 / 50,28 / 26 / 21,Air to Ait Cross Flow,23.4,51.6,640 x 320 x 640,25-3/16 x 12-9/16 x 25-3/16,4,125,4-23/25,1,Direct-Drive,1,Direct-Drive,2 / 1,Pre / MERV 13,275 x 280 x 7 / 275 x 277 x 50,10-13/16 x 11 x 1/4 / 10-13/16 x 10-7/8 x 1-15/16,-10~40 (14~104),3C x  0.82 (18),65 (100% Air Flow) / 69 (75% Air Flow) ,61 (100% Air Flow) / 65 (75% Air Flow) ,61 (100% Air Flow) / 66 (75% Air Flow) ,58 (100% Air Flow) / 61 (75% Air Flow) ,ERV,ZR1,ARV00903RA6,ARV00903RA6
ARV01203RA6,200,120,"1, 208/230, 60",0.62 / 0.56 / 0.28,79.2 / 71.4 / 30.5,200 / 200 / 100,120 / 120 / 60,100 / 70 / 50,30 / 28 / 22,0.65 / 0.59 / 0.32,83.6 / 75.6 / 35.9,200 / 200 / 100,120 / 120 / 60,100 / 70 / 50,30 / 28 / 22,Air to Ait Cross Flow,23.4,51.6,640 x 320 x 640,25-3/16'' x 12-9/16'' x 25-3/16'',4,125,4-23/25,1,Direct-Drive,1,Direct-Drive,2 / 1,Pre / MERV 13,275 x 280 x 7 / 275 x 277 x 50,10-13/16 x 11 x 1/4 / 10-13/16 x 10-7/8 x 1-15/16,-10~40 (14~104),3C x  0.82 (18),62 (100% Air Flow) / 65 (75% Air Flow) ,58 (100% Air Flow) / 61 (75% Air Flow) ,55 (100% Air Flow) / 61 (75% Air Flow) ,52 (100% Air Flow) / 58 (75% Air Flow) ,ERV,ZR1,ARV01203RA6,ARV01203RA6
