,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Refrigerant Charge (oz)##other##
LMU303HV,LMU303HV,U36A,-,Twin Rotary,30000,8.79,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2119,65,124.2 x 1,BLDC,Axial,32000,9.37,LMU303HV,63,138.9,3/8 x 4,9.52 x 4,1/4 x 4,6.35 x 4,2.3,2.3,"1, 208-230 , 60",3 x 12 (3.3),2800,9.52,6.35,R410A,10.46,10.59,64,66,51,54,-10~48,14~118,-20~18,-4~64,MULTI F,98.8
LMU363HV,LMU363HV,U36A,-,Twin Rotary,32800,9.61,37-13/32 x 32-27/32 x 13,950 x 834 x 330,Electronic Expansion Valve,2119,65,124.2 x 1,BLDC,Axial,36000,10.55,LMU363HV,63,138.9,3/8 x 4,9.52 x 4,1/4 x 4,6.35 x 4,2.6,2.7,"1, 208-230 , 60",3 x 12 (3.3),2800,9.52,6.35,R410A,11.88,12.40,64,66,51,54,-10~48,14~118,-20~18,-4~64,MULTI F,98.8
