,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Indoor Unit Total Capacity##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_High Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_High Gas Side (Heat Recovery)(mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant High Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Low Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZRUM036GSS0,U60A,2 x 18,Hermetically Sealed Scroll,36000,-,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",4238,-,0.124 x 2,Propeller,42000,-,-,31,ZRUM036GSS0,-,210,-,-,5/8,15.88,3/8,9.52,3/4,19.05,2.32,2.2,"1, 208-230,60",-,6,15.88,19.05,9.52,R32,-,-,-,23~122 (DB),-,-13~61 (WB),Multi V S R32
ZRUM048GSS0,U60A,2 x 18,Hermetically Sealed Scroll,48000,-,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",4238,-,0.124 x 2,Propeller,54000,-,-,31,ZRUM048GSS0,-,210,-,-,5/8,15.88,3/8,9.52,3/4,19.05,3.56,3.1,"1, 208-230,60",-,6,15.88,19.05,9.52,R32,-,-,-,23~122 (DB),-,-13~61 (WB),Multi V S R32
ZRUM060GSS0,U60A,2 x 18,Hermetically Sealed Scroll,60000,-,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",4238,-,0.124 x 2,Propeller,67000,-,-,32.8,ZRUM060GSS0,-,263,-,-,5/8,15.88,3/8,9.52,3/4,19.05,4.62,4.6,"1, 208-230,60",-,6.9,15.88,19.05,9.52,R32,-,-,-,23~122 (DB),-,-13~61 (WB),Multi V S R32
