,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
KNUFB181A,KNUFB181A,512(Max) / 477 / 406 / 335,-,TC,32,18000,5.3,40-5/32 x 7-3/4 x 13-3/8,1020 x 197 x 340,30 x 1,BLDC ,Cross Flow Fan,20000,5.9,ZMNR18GTCA0,-,30.4,1-1/4,32.0,1/2,12.7,1/4,6.35,3 x 18 / 2 x 18,-,-,"1, 208-230, 60",12.7,6.35,R32,0.58,-,46(Max) / 44 / 40 / 35,46(Max) / 44 / 40 / 35,1way CST
KNUFB121A,KNUFB121A,388 (Max) / 353 / 325 / 289,-,TC,32,12000,3.5,40-5/32 x 7-3/4 x 13-3/8,1020 x 197 x 340,30 x 1,BLDC ,Cross Flow Fan,15400,4.5,ZMNR12GTCA0,-,30.4,1-1/4,32.0,3/8,9.52,1/4,6.35,3 x 18 / 2 x 18,-,-,"1, 208-230, 60",9.52,6.35,R32,0.58,-,38(Max) / 35 / 33 / 30,38(Max) / 35 / 33 / 30,1way CST
KNUFB091A,KNUFB091A,353(Max) / 325 / 300 / 289,-,TC,32,9000,2.6,40-5/32 x 7-3/4 x 13-3/8,1020 x 197 x 340,30 x 1,BLDC ,Cross Flow Fan,12000,3.5,ZMNR09GTCA0,-,30.4,1-1/4,32.0,3/8,9.52,1/4,6.35,3 x 18 / 2 x 18,-,-,"1, 208-230, 60",9.52,6.35,R32,0.58,-,35(Max) / 33 / 31 / 30,35(Max) / 33 / 31 / 30,1way CST
KNMFB071A,KNMFB071A,325(Max) / 289 / 258 / 226,-,TC,32,7000,2.1,40-5/32 x 7-3/4 x 13-3/8,1020 x 197 x 340,30 x 1,BLDC ,Cross Flow Fan,8100,2.4,ZMNR07GTCA0,-,30.4,1-1/4,32.0,3/8,9.52,1/4,6.35,3 x 18 / 2 x 18,-,-,"1, 208-230, 60",9.52,6.35,R32,0.58,-,33(Max) / 30 / 28 / 25,33(Max) / 30 / 28 / 25,1way CST
