,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
LUU360HV,LUU360HV,U3,-,Scroll x 1,33200,9.7,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,"1,942 x 2",-,-,ECM (Electronically Commutated Motor),Propeller x 2,40000,11.7,LUU360HV,90.2,198.9,5/8,15.88,3/8,9.52,2.79,3.65,"1, 208-230 , 60",3 x 10,15.88,9.52,R410A,52,54,-,5~118,-,-4~64,SingleZone Outdoor
LUU420HV,LUU420HV,U3,-,Scroll x 1,42000,12.3,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,"1,942 x 2",-,-,Brushless Digitally Controller / Direct,Propeller x 2,47000,13.8,LUU420HV,95.7,210.9,5/8,15.88,3/8,9.52,3.91,3.95,"1, 208-230 , 60",3 x 10,15.88,9.52,R410A,52,54,-,5~118,-,-4~64,SingleZone Outdoor
LUU480HV,LUU480HV,U3,-,Scroll x 1,48000,14.0,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,"1,942 x 2",-,-,Brushless Digitally Controller / Direct,Propeller x 2,50000,14.6,LUU480HV,95.7,210.9,5/8,15.88,3/8,9.52,4.95,4.19,"1, 208-230 , 60",3 x 10,15.88,9.52,R410A,52,54,-,5~118,-,-4~64,SingleZone Outdoor
LUU601HV,LUU601HV,U3,-,R1 Scroll x 1,52000,15.2,37-13/32 x 54-11/32 x 13,"950 x 1,380 x 330",EEV,"1,942 x 2",-,-,Brushless Digitally Controller / Direct,Propeller x 2,56500,16.6,LUU601HV,95.7,210.9,5/8,15.88,3/8,9.52,4.49,4.73,"1, 208-230 , 60",3 x 10,15.88,9.52,R410A,52,54,-,5~118,-,-4~64,SingleZone Outdoor
