,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"LVN360HV4","1,100 / 1,000 / 900",-,NK,19.05,"14,000 ~ 36,000 ~ 44,000",-,25 x 55-3/16 x 21-1/4,635 x 1401 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"15,000 ~ 40,000 ~ 47,000",-,LVN360HV4,-,74.8,165,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,45 / 44 / 43,45 / 44 / 43,V AHU
"LVN420HV","1,260 / 1,100 / 1,000",-,NK,19.05,"17,000 ~ 42,000 ~ 48,000",-,25 x 55-3/16 x 21-1/4,635 x 1401 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"18,000 ~ 47,000 ~ 55,000",-,LVN420HV,-,74.8,165,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,48 / 45 / 44,48 / 45 / 44,V AHU
"LVN480HV","1,400 / 1,260 / 1,000",-,NK,19.05,"18,000 ~ 48,000 ~ 53,000",-,25 x 55-3/16 x 21-1/4,635 x 1401 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"19,000 ~ 56,000 ~ 60,000",-,LVN480HV,-,74.8,165,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,49 / 48 / 44,49 / 48 / 44,V AHU

