,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x H x D) (mm)##other##,Dimensions (W x H x D) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"LSN090HSV5",Wall Mounted,LSN090HSV5,S4NW09JL1DA,SJ ,837 x 308 x 189,32-15/16 x 12-1/8 x 7-7/16,16.0,5/8,21.5,27/32,9.52,3/8,6.35,1/4,1_208/230_60,4 x 1.0,4 x 18,2.9,3.5,13.0 / 11.0 / 9.0 / 5.5,459 / 338 / 317 / 194,13.0 / 11.0 / 9.0 / 6.5,459 / 338 / 317 / 229,2.64,"9,000",3.19,"10,900",620,710,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,30,8.3,18.3,R410A,- / 41 / 35 / 25 / 21,- / 41 / 35 / 26
"LSN120HSV5",Wall Mounted,LSN120HSV5,S4NW12JL1DA,SJ ,837 x 308 x 189,32-15/16 x 12-1/8 x 7-7/16,16.0,5/8,21.5,27/32,9.52,3/8,6.35,1/4,1_208/230_60,4 x 1.0,4 x 18,4.5,4.7,13.0 / 11.0 / 9.0 / 5.5,459 / 338 / 317 / 194,13.0 / 11.0 / 9.0 / 6.5,459 / 338 / 317 / 229,3.5,"12,000",3.98,"13,600",960,"1,040",Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,30,8.3,18.3,R410A,- / 41 / 35 / 25 / 21,- / 41 / 35 / 26
