,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Minimum Circuit Ampacity (MCA) (A)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"LSU090HSV5",Wall Mounted,LSU090HSV5,S4UW09JLRDA,UL2,770 x 545 x 288,30-5/16 x 21-15/32 x 11-11/32,9.52,3/8,6.35,1/4,10,15,1_208/230_60,3 x 2.5,3 x 12,4 x 1.0,4 x 18,2.9,3.5,33,1165,2.64,9000,3.19,10900,620,710,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,15,49.2,33.6,74.1,-10 [-18 ²] ~ 48 (DB),14 [0 ²] ~ 118 (DB),-20 ~ 18.3 (WB),-4 ~ 65 (WB),3 / 7.5 / 25,9.8 / 24.6 / 82,12.5,41,R410A,1000,35.3,20,0.22,47,51
"LSU120HSV5",Wall Mounted,LSU120HSV5,S4UW12JLRDA,UL2,770 x 545 x 288,30-5/16 x 21-15/32 x 11-11/32,9.52,3/8,6.35,1/4,10,15,1_208/230_60,3 x 2.5,3 x 12,4 x 1.0,4 x 18,4.5,4.7,33,1165,3.5,12000,3.98,13600,960,1040,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,15,49.2,33.6,74.1,-10 [-18 ²] ~ 48 (DB),14 [0 ²] ~ 118 (DB),-20 ~ 18.3 (WB),-4 ~ 65 (WB),3 / 7.5 / 25,9.8 / 24.6 / 82,12.5,41,R410A,1000,35.3,20,0.22,47,51


