,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Independent Unit##other##,Indoor Unit Model Max Quantity##other##,Indoor Unit Total Capacity##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_High Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_High Gas Side (Heat Recovery)(mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(inch)##other##,Pipe Connection_Low Gas Side (Heat Recovery)(mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ARUN072BSS5,U80A,2 x 18(Only Comm. Cable),Hermetically Sealed Scroll,69,20.223,43.0 x 64.0 x 15.0,"1,090 x 1,625 x 380",7416,210,0.25,Axial Flow Fan,81,22.567,ARUN072BSS5,13,50~130%,24.4,ARUN072BSS5,158,348,3/4,19.05,-,-,3/8,9.52,-,-,5.798,5.938,"3, 208-230 , 60",-,13.2,19.05,9.52,R410A,55,57,-,23 to 122,-,-13 to 61,Multi V S
ARUN096BSS5,U80A,2 x 18(Only Comm. Cable),Hermetically Sealed Scroll,92,26.964,43.0 x 64.0 x 15.0,"1,090 x 1,625 x 380",7416,210,0.25,Axial Flow Fan,108,30.188,ARUN096BSS5,16,50~130%,25.7,ARUN096BSS5,158,348,7/8,22.22,-,-,3/8,9.52,-,-,8.363,9.147,"3, 208-230 , 60",-,13.2,22.22,9.52,R410A,59,60,-,23 to 122,-,-13 to 61,Multi V S
