,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
AUUW18GH0,LUU180HHV,U4,-,Scroll x 1,Duct:18000 / VAHU:18000 / CST:18000,Duct:5.2 / VAHU:5.2 / CST:5.2,37-13/32 x 32-53/64 x 13,950 x 834 x 330,Electronic Expansion Valve,2048,58,124,BLDC,AXIAL,Duct:20000 / VAHU:20000 / CST:20000,Duct:5.8 / VAHU:5.8 / CST:5.8,AUUW18GH0,60.5,133.4,5/8,15.88,3/8,9.52,1.44,1.82,"1, 208-230 , 60",3 x 12(3.3),2000,15.88,9.52,R410A,6.4,8.1,-,-,51,52,-10~48,14~118,-25~18,-13~64.4,SingleCAC
AUUW24GH0,LUU240HHV,U4,-,Scroll x 1,Duct:23000 / VAHU:24000 / CST:24000,Duct:6.7 / VAHU:7.0 / CST:7.0,37-13/32 x 32-53/64 x 13,950 x 834 x 330,Electronic Expansion Valve,2048,58,124,BLDC,AXIAL,Duct:27000 / VAHU:27000 / CST:27000,Duct:7.9 / VAHU:7.9 / CST:7.9,AUUW24GH0,60.5,133.4,5/8,15.88,3/8,9.52,1.84,2.08,"1, 208-230 , 60",3 x 12(3.3),2000,15.88,9.52,R410A,8.2,9.2,-,-,51,52,-10~48,14~118,-25~18,-13~64.4,SingleCAC
