,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"LVN181HV4",640 / 580 / 480,-,NJ,19.05,"7,200 ~ 18,000 ~ 23,000",-,18 x 48-11/16 x 21-1/4,457 x 1236 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"8,000 ~ 20,000 ~ 24,000",-,LVN181HV4,-,58.5,123.5,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,35 / 33 / 30,35 / 33 / 30,V AHU
"LVN241HV4",710 / 640 / 480,-,NJ,19.05,"9,600 ~ 24,000 ~ 30,000",-,18 x 48-11/16 x 21-1/4,457 x 1236 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"10,800 ~ 27,000 ~ 30,000",-,LVN241HV4,-,58.5,123.5,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,36 / 34 / 30,36 / 34 / 30,V AHU
"LVN361HV4",990 / 880 / 800,-,NJ,19.05,"14,400 ~ 36,000 ~ 39,000",-,18 x 48-11/16 x 21-1/4,457 x 1236 x 540,-,Brushless Digitally Controller / Direct,Sirocco x 1,"16,000 ~ 40,000 ~ 43,000",-,LVN361HV4,-,58.5,129,3/4,19.05,5/8,15.88,3/8,9.52,4 x 18,-,-,"1, 208-230, 60",15.88,9.52,R410A,-,-,44 / 41 / 39,44 / 41 / 39,V AHU

