,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##
ZRNU123TRAA,307 / 283 / 247,-,TR,32,12300,3.60,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43,BLDC,Turbo Fan,4000,4.00,0.4,-,ZRNU123TRAA,13.2,29.1,1-1/4,32,3/8,9.52,1/4,6.35,17/15/13,-,"1,208/230, 60",9.52,6.35,R32,0.25,32 / 30 / 27,Mini 4Way
ZRNU073TRAA,265 / 247 / 212,-,TR,32,7500,2.20,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43,BLDC,Turbo Fan,2500,2.50,0.4,-,ZRNU073TRAA,12.0,26.5,1-1/4,32,3/8,9.52,1/4,6.35,13/12/11,-,"1,208/230, 60",9.52,6.35,R32,0.25,29 / 27 / 26,Mini 4Way
ZRNU093TRAA,283 / 265 / 251,-,TR,32,9600,2.80,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43,BLDC,Turbo Fan,3200,3.20,0.4,-,ZRNU093TRAA,13.2,29.1,1-1/4,32,3/8,9.52,1/4,6.35,14/13/12,-,"1,208/230, 60",9.52,6.35,R32,0.25,30 / 29 / 27,Mini 4Way
ZRNU053TRAA,265 / 247 / 212,-,TR,32,5500,1.61,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43,BLDC,Turbo Fan,1800,1.80,0.4,-,ZRNU053TRAA,12.0,26.5,1-1/4,32,3/8,9.52,1/4,6.35,13/12/11,-,"1,208/230, 60",9.52,6.35,R32,0.25,29 / 27 / 26,Mini 4Way
